|  |
| --- |
| **Complete Every Time Prior To Use** |
| **Fences and gates**: |
| No broken boards, protrusions, tripping hazards, sharp points, nails. |
| No broken rails, loose panels or broken/loose posts. |
| Gates swing freely and shut properly. Tub ratchet locks working and holding |
| Treads on loading chute/ramp are solid, and free of debris/shadow casting objects. |
| Escape routes are free of obstructions. |
| **Processing Chute** |
| Free of debris & distracting/balking/shadow casting objects. |
| Anti-back up devices/pole/bars in place |
| Tail/end gate, side rails palpation doors, headgate: all parts move freely |
| Gears and locking parts on levers engage, catch and hold |
| **Catwalks** |
| Secure, with no gaps between boards or surfaces. |
| Boards are free of rot, debris, and slipping/tripping hazards. |
| **Squeeze: (& Scale if applicable)** |
| Free motion and movement auto catch working properly |
| Secure to posts and ground, floor/ground surface clear and solid |
| No tripping hazards around head gate/squeeze area |
| Headgate moves freely, quietly, and locks/unlocks |
| Deck is clean and in good repair, sharps stored properly, vaccinations and medications safely and securely stored for use |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Date** | **Checked by** | **Check**  **If OK** | **Repairs Needed** | **Date Repaired** | **Repaired by** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |