

|  |
| --- |
| **Company Information** |
| **Company Name:** |  |
| **Workplace Location:** |  |
| **Name of Safe Work Practice:**   | Farm and Field Work | **Release Date:** |  |
| **Safe Work Practice #:** |  | **Revision Date:**  |  |
| **Management Signature:** |  | **Date of Approval:** |  |
| **Instructions** |
| This safe work practice must be reviewed annually or any time the task, equipment, or materials change. |
| Do **NOT** perform the duties listed in this *Safe Work Practice* until you have been appropriately trained and authorized to do so by your supervisor |
| **Personal Protective Equipment:** |
| Appropriate clothing for the weather, safety boots, ear protection (open cab), eye protection (open cab), high vis vest (if working around tractor), gloves |
| **Hazards:** |
| * Rollover
* PTO entanglement
 |
| **Practice for Multiple Lockout:** |
| 1. Always use belt with approved ROPS
2. Remain in the seat during operation.
3. Use only approved implements with tractor.
4. Read tractor and implement manuals prior to use.
5. Before starting make sure all levers and controls are in neutral or disengaged and park brake is on.
6. Do not permit anyone but the operator to ride on the tractor.
7. Disengage PTO, shut off the engine and apply the parking brake before getting off the tractor.
8. Do not park tractor on steep slopes.
9. PTO must be guarded.
10. Hitch and pull only with the designed drawbar.
11. Always slow prior to a sharp turn.
12. Drive in a manner that will avoid braking in the curve.
13. Utilize “Slow Moving Vehicle” sign on public roadways.
14. If working alone, ensure working alone procedure is followed.
15. Review field maps to identify high risk areas.
 |