|  |
| --- |
| **Company Name:** |
| **Location:** |
| **Name of Inspector(s):** |
| **Date of Inspection:** |
| **Inspection Items** |
| A facemask (respirator with HEPA dust filter) is available where workers may be exposed to damp or moldy hay or sawdust, or dust from feed. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| If an elevator or conveyor is used, all mechanisms, belts, and other moving parts are completely guarded. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| All PTO and other equipment guards are in place on the mixing wagon. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| Sturdy railings have been built around all edges and drop- offs, wherever possible. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| All ladders are sturdy and well secured. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| If a tower silo is used, access to the ladder is restricted. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| If a tower silo is used, signs are posted to warn of the hazards of silo gas. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| If a bunker silo is used, ventilation is good in all the areas where people may be working. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| If a bunker silo is used, the walls are sturdy enough for the combined weight of the silage and the equipment used to compact it. | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
|  | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
|  | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
|  | * Yes
* No
* N/A
 |
| Corrective Action: | Who is Responsible: |
| Action Date: |
| **Other Notes:**  |