**Disclaimer:** This resource is intended for guidance and employers are advised to customize this document or design their own to meet their business needs and legal obligations. Once customized from its original content this disclaimer may be removed to function as part of your Safety Program. This resource does not relieve persons using it from their responsibilities under applicable legislation. If you need assistance contact us at www.AgSafeBC.ca

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Company:** | | | **Workplace Location:** | |
| **Prepared by:** | | | **Date:** | |
| **TASK** | **HAZARD** | **LEVEL OF RISK** | | **CONTROL METHOD** |
| **Remove cart puller from charger and back up to carts that are to be attached** | Run over- bystander hazard | **Low/ Moderate** | | * Ensure directional path is clear * Make workers in the area aware of work before it is commenced * Sound horn when backing up |
| Crushed/struck by carts- bystander hazard | **Low/ Moderate** | | * Ensure directional path is clear- ensure no workers are standing behind or in between carts * Make workers in the area aware of work before it is commenced * Sound horn when backing up |
| Crush/Pinch- attaching puller to carts | **Low/ Moderate** | | * Instruct workers never to put hands in pinch points |
| **Once train of carts is attached, slowly drive away in straight line of travel** | Cart tip over | **Moderate** | | * Instruct workers to drive slowly and take corners at low rate of speed |
| Crushed/struck by carts- bystander hazard | **Low/ Moderate** | | * Make workers in the area aware of work before it is commenced |
| Run over- bystander hazard | **Low/ Moderate** | | * Sound horn when backing up |
| **Unhook carts and return cart puller to designated charging station** | Cart tip over | **Moderate** | | * Instruct workers to drive slowly and take corners at low rate of speed. Instruct workers to come to a slow stop. |
| Crushed/struck by carts- bystander hazard | **Low/ Moderate** | | * Make workers in the area aware of work before it is commenced |
| Run over- bystander hazard | **Low/ Moderate** | | * Sound horn when backing up |
| Crush/Pinch- un attaching puller to carts | **Low/ Moderate** | | * Instruct workers never to put hands in pinch points |
| **Other Recommendations:**  Before use, conduct a pre-trip inspection on electric cart puller, if not safe for use, report to a supervisor and put out of service. | | | | |