

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Competency:** | | **Fencing** | | | | | | | | | |
| **Company Name:** | | | |  | | | | **Date:** |  | | |
| **Workplace Location:** | | | | |  | | | | | | |
| **Worker Name:** | | |  | | | **Evaluator:** |  | | | | |
| **Step** | **Activity** | | | | | | | | | **Pass** | **Fail** |
| **1** | Can identify appropriate PPE to wear | | | | | | | | |  |  |
| **2** | Review manuals of chainsaw/auger/post driver/tractor (whatever equipment is being used) | | | | | | | | |  |  |
| **3** | If required check for underground hazards and services (BC One Call: 1-800-474-6886) | | | | | | | | |  |  |
| **4** | Identify treated vs. untreated posts and rails and handle accordingly | | | | | | | | |  |  |
| **5** | Utilizes correct technique and posture while driving posts manually (post pounder or maul) | | | | | | | | |  |  |
| **6** | If using a post driver or auger ensure that:   * Appropriate tractor is selected. * Inspects prior to use. * Ensure PTO shaft is guarded. * Can attach and detach the post driver/auger. * Transports with the hammer lowered (post driver). * Tractor is parked and braked before use. * Drive belts, pulleys, chains and sprockets are guarded. * Does not use hands to steady and guide the post (post driver). | | | | | | | | |  |  |
| **7** | Is aware of wire recoil when cutting | | | | | | | | |  |  |
| **8** | Utilizes a wire dispenser when rolling out wire | | | | | | | | |  |  |
| **9** | Does not over tension wire | | | | | | | | |  |  |
| **10** | Cleans up area of all debris after fencing section is complete | | | | | | | | |  |  |
| **11** | Knows supervisor and contact information | | | | | | | | |  |  |
| **12** | Knows where first aid kits are, who is the first aid attendant and first aid contact information | | | | | | | | |  |  |
| **13** | Worker can identify and utilizes appropriate PPE | | | | | | | | |  |  |
| **14** | Worker uses appropriate SWPs | | | | | | | | |  |  |
| **15** |  | | | | | | | | |  |  |
| **16** |  | | | | | | | | |  |  |
| **17** |  | | | | | | | | |  |  |
| **Comments/Deficiencies:**  \*\*Report all deficiencies in worker deficiency checklist\*\* | | | | | | | | | | | |
| **DO NOT commence work if you notice something is wrong - Contact supervisor/manager immediately.** | | | | | | | | | | | |