|  |  |
| --- | --- |
| **Presented by:** | **Date of meeting:** |
| **Meeting start time:** | **Meeting end time:** |
| **Health and safety issues discussed** | |
| * Keep work areas and shops clean, dry, and tidy and put tools and equipment away after use. * Use footwear with good tread. * Be aware of weather and ground conditions, ice, mud, wet, uneven ground, etc. * Watch for manure, spilled feed. Clean up when found. * Check handling facilities for good repair – no protruding boards or items in walking / working areas. * Use caution around panels fences and gates, and use gates rather than climbing over fences & panels. * Keep feed bunks clear of snow and ice. * Use caution carrying objects over uneven or steep terrain. * Hoses, ropes, twine, cables, extension cords etc.   + When not in use, roll up and store properly.   + When being used, be aware of placement. Keep away from walking areas if possible. * Stairs should be clear of obstacles and well lit. Use handrail when available. * Ladders: use correct ladder for the job, set up properly and securely. Use 3-point contact on ladders. * Pick up dropped items as soon as possible and follow spill clean-up process for liquid spills. * Use steps and 3-point contact when getting on and off mobile equipment. | |
| **Review procedures & workplan** | |
|  | |
| **Worker comments / feedback:** | |
|  | |



To be signed by all employees, contract workers, clients and others who participated in the safety talk prior to commencing work.

|  |  |
| --- | --- |
| **Who Attended:** | |
| **PRINT NAME** | **SIGNATURE** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |