**PPE Requirements**

1. Sturdy, snug fitting clothing
2. Gloves
3. Steel toed boots
4. Safety glasses
5. Hearing protection

**General Safety Practices**

1. Read manual to ensure comfort with all controls, safety stickers and operation of the BaleBuster.
2. Ensure all guards and shields are in place.
3. Perform “walk around” of machine to inspect for damage or wear.
4. Attach BaleBuster to tractor PTO
5. Load bale into BaleBuster
6. Adjust deflector to desired position
7. Engage PTO
8. Engage bale conveyor
9. Ensure no bystanders are near.
10. Ensure PTO is disconnected before any maintenance is performed on the BaleBuster.