|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Company:** | | | | **Workplace Location:** |
| **Prepared by:** | | | | **Date:** |
| **TASK** | **HAZARD** | **LEVEL OF RISK** | **CONTROL METHOD** | |
| **As a team roll out cloth across designated greenhouse bay** | Sprain/Strain from lifting and rolling cloth | **Moderate** | * Instruct workers to practice proper lifting technique. * PPE- non-slip footwear and knee pads. | |
| Dirt/Debris in eyes | **Low/Moderate** | * PPE- eye protection. | |
| Slip/Trip | **Low/Moderate** | * Ensure greenhouse bay is clear of holes and debris. * PPE- non-slip footwear. | |
| **Smooth cloth. Using staple gun tack the cloth down every 6-8 feet.** | Puncture from staple gun. | **Moderate/High** | * Ensure workers have been instructed on use of nail gun. * PPE- Impact resistant safety glasses. * Ensure workers keep hands away from firing area. * Ensure workers never staple into a surface that cannot be penetrated by the staple. | |
| **Other Recommendations:** Inspect all tools before use. Be aware of locations of water and electrical lines before using staple gun. | | | | |

**Disclaimer:** This resource is intended for guidance and employers are advised to customize this document or design their own to meet their business needs and legal obligations. Once customized from its original content this disclaimer may be removed to function as part of your Safety Program. This resource does not relieve persons using it from their responsibilities under applicable legislation. If you need assistance contact us at www.AgSafeBC.ca